|  |
| --- |
| **Shanghai Goodview Electronic Technology Co., Ltd.** |
| **Specification** |
| M75GUQ |



**Sign and Date by: \_\_\_\_\_\_\_\_\_\_\_ Sign and Date by: \_\_\_\_\_\_\_\_\_\_\_\_**

**Customer Good View**

**Content**

Content..............................................................................................................................................................1

[Chapter I. Revision History 2](#_Toc23325633)

[Chapter II. Summary 3](#_Toc23325634)

[2.1. Statement 3](#_Toc23325635)

[2.2. Safety instructions 4](#_Toc23325636)

[Chapter III. Product Parameter 5](#_Toc23325637)

[3.1. Main Technical Parameters 5](#_Toc23325638)

[3.1.1 LCD Panel Technical Parameters 7](#_Toc23325639)

[3.2. Input Signal 8](#_Toc23325640)

[3.2.1. HDMI Port 8](#_Toc23325641)

[3.2.2 VGA Port 8](#_Toc23325642)

3.3. Specification Overview 9

[3.3.1. AC Input Electrical Characteristics 9](#_Toc23325643)

[3.3.2. Green mode function 9](#_Toc23325644)

[3.4. External Interface Portion 9](#_Toc23325645)

[Chapter IV. Mechanical Portion 1](#_Toc23325646)0

[4.1. Outline drawing 10](#_Toc23325647)

[Chapter V. Packaging Portion 11](#_Toc23325648)

[5.1. Packing Size 1](#_Toc23325649)1

[5.2. Packaging Drawings 1](#_Toc23325650)1

[5.3. Nameplate 12](#_Toc23325651)

[5.4. Labels 12](#_Toc23325652)

[Chapter VI. Environmental Requirement 13](#_Toc23325654)

[6.1. Operating Temperature 1](#_Toc23325655)3

[6.2. Storage Temperature 13](#_Toc23325656)

[Chapter VII. ID Rendering 1](#_Toc23325657)4

[7.1. Six Sides Figure 14](#_Toc23325658)

[7.2. Front View 14](#_Toc23325659)

[7.3. Back View 15](#_Toc23325660)

[7.4. End View 15](#_Toc23325661)

[7.5. Interface Rear View 16](#_Toc23325662)

# Revision History

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Parts No.** | **Version** | **Revision History** | **Date** | **Written by** | **Auditing** | **Approval** |
| 1440274 | V1.0 | First issue | 2022/12/30 | 张梦丽 | / |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

# Summary

## 2.1. Statement

All parts of this product, including accessories and software, all the intellectual property right are owned by Shanghai Goodview Electronic Technology Co., Ltd. (hereinafter refers to "Goodview") or authorizes the relevant subjects xxxx to use. Without the permission of the right subjects, no copying or translation is allowed.

There is no any form of guarantee, position expression or other implication in this manual, if there is any direct or indirect loss of data, loss of profits or termination of business caused by the product information mentioned in this manual, Goodview and its employees are not liable for it. In addition to this, the product specifications and information mentioned in this manual are only for reference and will be updated at any time without further notice. Faults or damages caused by the following factors are not covered by free warranty:

* Damage caused by natural disasters (floods, fires, earthquakes, lightning strikes, typhoons, etc.), force majeure or inadvertent use of man-made operations.
* Self-assemble, repair, or send the product to a maintenance shop not authorized or certified by Goodview for inspection and repair.
* Damages and faults caused by users who may or request a third party to modify, repair, alter specifications and install, add and expand parts that are not sold, authorized or approved by our company without authorization.
* Usage problems and faults caused by improper installation and setting of software by users themselves.
* Problems and malfunctions caused by computer viruses.
* Warranty identification label of our company is torn or unrecognizable.
* Other problems and faults caused by abnormal use.

The product names mentioned in the user's manual are only for identification, and these names may belong to registered trademarks or copyrights of other companies.

Goodview reserves the right to change any or all specifications without notice. The information contained in this document is subject to change without notice.

For the latest upgrade information of product specifications, please call to Shanghai Goodview Electronic Technology Co., Ltd.

## 2.2. Safety instructions

**Safety of Electrical**

* In order to avoid serious damage caused by possible electric shock, please remove the power cord of the equipment temporarily from the power socket before moving the equipment
* When you want to add or remove the hardware device in the system, you must connect the data line of the device first and then the power line. If possible, unplug the power cord of the device before installing the hardware device.
* Before you connect or unplug any data lines from the module, make sure that all the power lines have been unplugged beforehand.
* Before using an extension card or an adapter card, we suggest that you seek for professional assistance first. These devices may interfere with the grounding circuit.
* Make sure that the voltage settings of the power supply have been adjusted to the voltage standard values used in the country/region. If you are not sure what the supply voltage value is in your area, please ask the local power company personnel nearby.
* If the power supply is damaged, please do not attempt to repair it by yourself. Please seek the help of professional technical service personnel.

**Safety in operation**

* Before you install modules and add hardware devices, be sure to read the relevant information provided in this manual in detail.
* Before using the product, make sure that all the data lines and power lines are connected correctly. If you find any defects, please contact Goodview as soon as possible.
* In order to avoid electrical short circuit, make sure that all unused screw, paper clip and other parts are put away, and do not leave them on the module or in the equipment.
* Dust, moisture and drastic temperature changes will affect the life of the motherboard, so please try to avoid placing them in these places.
* Do not place the equipment in a place that is easy to shake.
* If there are any technical problems in the use of this product, please contact the technicians who have been verified or experienced.

# Product Parameter

## 3.1. Main Technical Parameters

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **NO** | **Subtype** | **Name** | | **Parameter** | **Unit** | **Note** |
| 1 |  | Panel | | 75 inches LED backlight |  |  |
| 2 | Product  Parameter | Product size (mm) | | 1685.6(H)×963.7 (V)×81.6(D) | mm |  |
| 3 | Active size (mm) | | 1650.2(H)×928.3(V) | mm |  |
| 4 | Color | | Black |  |  |
| 5 | Weight (Gross) | | 48.15 | KG |  |
| 6 | Weight (Net) | | 34.65 | KG |  |
| 7 | Speaker | | 2×10W | Watt |  |
| 8 | Display direction | | ☑Vertical ☑Horizontal |  |  |
| 9 | OSD Language | | Chinese\English |  |  |
| 10 | Play mode | | ☑Horizontal ☑Vertical☑Split display ☑Play List |  |  |
| 11 | Multimedia transmission | | USB,LAN,WAN |  |  |
| 12 | Function | Smart volume | | Time sharing volume |  |  |
| 13 | Watch dog | | Support |  |  |
| 14 | Timer | | Multi-period timing switch |  |  |
| 15 |  | Management software | | B/S framework: GTV Information Distribution System |  |  |
| 16 | Core | CPU | | Quad-core A55 |  |  |
| 17 | GPU | | Mali G52MP2 |  |  |
| 18 | Memory | | 4GB |  |  |
| 19 | Storage | | 32GB eMMc |  |  |
| 20 | Operation System | | Android11 |  |  |
| 21 | Multimedia | Picture | Extension | \*.jpg, \*.jpeg, \*.bmp, \*.png |  |  |
| 22 | Audio | Extension | \*.mp3 |  |  |
| 23 | Video | Extension | MPEG1、MPEG2、MPEG4、WMV、MKV、AVI、TS、flv |  |  |
| Encoder | MPEG-1        bitrate<20Mbps  MPEG-2        bitrate<20Mbps MPEG-4        bitrate<20Mbps H.264            bitrate<20Mbps AVC              bitrate<20Mbps VC-1             bitrate<20Mbps RM        bitrate<10Mbps |
| 24 | Text | Extension | .txt |  |  |
| 25 | HTMI 5 | | Support |  |  |
| 26 |  | VESA standard | | 800x600 |  |  |
| 27 | Installation mode | | VESA |  |  |
| 28 | Installation |  | | 1. National standard power cord 3m×1  2. Remote control × 1  3. AAA battery × 2  4. WIFI module × 1  5. HDMI cable 3mx1  6. Warranty card certificate x1  7. User manual x1 |  |  |
| 29 | Certification |  | | CCC CECP CE FCC |  |  |

### 3.1.1 LCD Panel Technical Parameters

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | | **Symbol** | **Parameter** | | | Unit | Note |
| **Min** | **Typ** | **Max** |
| LCD Panel Size | |  | - | 75 | - | inches | |  | | --- | | Led backlight | |
| Active Screen Size | |  | 1650.2(H)×928.3(V) | | | mm |  |
| Pixel Format | |  | 3840×2160 | | | Pixels |  |
| Panel Luminance | |  |  | 500 | - | cd/m2 |  |
| Product Luminance | |  |  | 500 | - | cd/m2 |  |
| Contrast Ratio | | CR |  | 1200 | - |  |  |
| Color Depth | |  | 10bit, 1.07 Billion colors | | |  |  |
| Pixel Pitch | |  | 0.4296×0.4296 | | | mm |  |
| Color temperature | |  | - | - | - | K |  |
| Color Gamut | |  | - | 72% | - |  |  |
| Response Time | | G to G BW | - | 8 |  | ms |  |
| Backlight Life Time | |  | - | 50000 | - | Hrs |  |
| Viewing Angle | Xaxis,right=0° | R | 89 | - | - |  |  |
| x axis, left=180° | L | 89 | - | - |  |
| y axis, up =90° | U | 89 | - | - |  |
| yaxis, down=270° | D | 89 | - | - |  |

## 3.2 Input Signal

### 3.2.1 HDMI Port

|  |  |
| --- | --- |
| Resolution | Refresh |
| 1024x768 | @60Hz/50Hz |
| 1600x900 | @60Hz/50Hz |
| 1280x800 | @60Hz/50Hz |
| 1280x720 | @60Hz/50Hz |
| 1280x1024 | @60Hz/50Hz |
| 1360x768 | @60Hz/50Hz |
| 1366x768 | @60Hz/50Hz |
| 1440x900 | @60Hz/75Hz |
| 1680x1050 | @60Hz/50Hz |
| 1920x1080 | @60Hz/50Hz |

### 3.2.2 VGA Port

|  |  |
| --- | --- |
| Resolution | Refresh |
| 1024x768 | @60Hz/50Hz |
| 1600x900 | @60Hz/50Hz |
| 1280x800 | @60Hz/50Hz |
| 1280x720 | @60Hz/50Hz |
| 1280x1024 | @60Hz/50Hz |
| 1360x768 | @60Hz/50Hz |
| 1366x768 | @60Hz/50Hz |
| 1440x900 | @60Hz/75Hz |
| 1680x1050 | @60Hz/50Hz |
| 1920x1080 | @60Hz/50Hz |

## 3.3 Specification Overview

### 3.3.1 AC Input Electrical Characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Item | Symbol | Values | | | Unit | Note |
| Min | Typ | Max |
| AC Power Input Voltage | AC IN | 100 | 220 | 240 | VAC |  |
| AC Power Input Current |  | - | - | 4.5A | AAC |  |
| Power Consumption |  | - | - | 450 | Watt |  |

### 3.3.2 Green mode function


|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Item | Symbol | Values | | | Unit | Note |
| Min | Typ | Max |  |
| Stand-by power consumption |  | ~~-~~ | ~~-~~ | 0.5 | Watt |  |

## 3.4 External Interface Portion

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **NO** | **Subtype** | **Name** | **Number** | **Parameter** |
|  | Ac input | Coupler | ×1 | Torx tail |
|  | AC Switch | ×1 | Rocker switch |
|  | Input/output  Terminals | HDMI IN | ×3 | Supports HDCP 2.1, CEC, ARC (HDMI 1), up to 4K@60Hz |
|  | Type-c | ×1 | Video, audio, external charging 65W, LAN network sharing |
|  | HDMI OUT | x1 | Maximum support 4K@60Hz , only supports HDMI IN signal output, not Android channel and HDMI 3 signal output |
|  | Audio out | x1 | 3.5mm headphone connector |
|  | SPDIF | x1 | PCM output format |
|  | Control  Terminals | RJ45 IN | ×1 | 10M/100M/1000Mbps |
|  | RJ45 OUT | ×1 | 10M/100M/1000Mbps |
|  | WiFi | ×1 | 2.4/5G WiFi IEEE802.11b/g/n |
|  | USB2.0 | ×1 | For system upgrade |
|  | USB3.0 | ×1 | External USB flash disk, mouse and other peripherals |
|  | RS232 | ×1 | Baud rate 115200 |


# VI.Mechanical Portion

## 4.1 Outline drawing



# Packaging Portion


## 5.1 Packing Size



## 5.2 Packaging Drawings

### 

## 5.3 Nameplate



## 5.4 Labels



# Environmental Requirement

## 6.1 Operating Temperature


|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Item | Symbol | Values | | | Unit | Note |
| Min | Typ | Max |
| Operating Temperature | Hop | 0 | - | 40 | ℃ |  |
| Operating Ambient Humidity | Hop | 10% | - | 80% | %RH | Relative humidity (non-condensing). |

## 6.2 Storage Temperature

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Item | Symbol | Values | | | Unit | Note |
| Min | Typ | Max |
| Storage Temperature | HST | -10 | - | 55 | ℃ |  |
| Storage Humidity | HST | 10% | - | 80% | %RH | relative humidity (non-condensing). |

# ID Rendering


## 7.1 Six Sides Figure



## 7.2 Front view



## 7.3 Back view



## 7.4 End View



## 7.5 Interface Rear View

